Campbell Scientific Data Logger notes

|  |  |  |
| --- | --- | --- |
| Contact | Phone number | email |
| Water Resources General Number | 435-227-9050 |  |
| David Odd | 435-227-9522 | dodd@ |
| Ken Conner | 435-227-9842 | kconner@ |
| Terrell Fletcher (group manager) | 435-227-9522 |  |
| Douglas Neff | 435-227-9602 | dneff@campbellsci.com |
|  |  |  |

To connect to SC105

* RS 232 side to null modem to USB/serial converter
* CS I/O side to data logger
* Click ‘Connect’ in Device Configuration Utility, then hit button on side of SC105
* Make changes to either the RS232 side or the CS I/O side, then apply
* It will provide a summary screen, hit OK, then it will automatically disconnect.

Direct connection to Data Logger

* Connection will go through the SC105
* Plug null modem into RS232 side of SC105 (unplug 950 data cable if plugged in)
* Direct connection “site” in LoggerNet needs to be set at correct baud rate (should be 19.2k on the RS232 side)
* Click connect and should connect almost immediately
* Disconnect when done